## Uses of Class
tw.com.prolific.driver.pl2303g.PL2303GDriver.BaudRate

- - ### Uses of PL2303GDriver.BaudRate in tw.com.prolific.driver.pl2303g

    Methods in tw.com.prolific.driver.pl2303g that return PL2303GDriver.BaudRate
    Modifier and Type | Method and Description
    --- | ---
    `static PL2303GDriver.BaudRate` | PL2303GDriver.BaudRate.`valueOf(java.lang.String name)` Returns the enum constant of this type with the specified name.
    `static PL2303GDriver.BaudRate[]` | PL2303GDriver.BaudRate.`values()` Returns an array containing the constants of this enum type, in the order they are declared.

    Methods in tw.com.prolific.driver.pl2303g with parameters of type PL2303GDriver.BaudRate
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | PL2303GDriver.`InitByBaudRate(PL2303GDriver.BaudRate R)` Open an PL2303G USB Device by BaudRate (The stop bit is 1, The parity bit is none, The Flow Control is none), the Timeout Constant of read and write is 100ms
    `boolean` | PL2303GDriver.`InitByBaudRate(PL2303GDriver.BaudRate R, int TimeoutConstant)` Open an PL2303G USB Device by BaudRate (The stop bit is 1, The parity bit is none, The Flow Control is none)
    `boolean` | PL2303GDriver.`InitByPortSetting(PL2303GDriver.BaudRate R, PL2303GDriver.DataBits D, PL2303GDriver.StopBits S, PL2303GDriver.Parity P, PL2303GDriver.FlowControl F)` Open an PL2303G USB Device by BaudRate, Data bit, stop bit, parity bit and Flow Control
    `boolean` | PL2303GDriver.`Set_PL2303_BaudRate(PL2303GDriver.BaudRate R)` Open an PL2303G USB Device by BaudRate
    `int` | PL2303GDriver.`setup(PL2303GDriver.BaudRate R, PL2303GDriver.DataBits D, PL2303GDriver.StopBits S, PL2303GDriver.Parity P, PL2303GDriver.FlowControl F)` Setup basic communication parameters on PL2303G chip